Supporting Information

Evaluation of Mechanical Properties and Hydrophobicity of Room-Temperature, Moisture-Curable Polysilazane Coatings

Ying Zhan a, \*, Ralf Grottenmüller b, Wei Li a, Farhan Javaid a, c, Ralf Riedel a, \*

a. Institute of Materials and Earth Sciences, Technical University of Darmstadt, D-64287 Darmstadt, Germany

b. Merck KGaA, D-64293 Darmstadt, Germany

c. School of Chemical and Materials Engineering, National University of Sciences & Technology, 44000 Islamabad, Pakistan

\*. Corresponding authors: [ying.zhan@tu-darmstadt.de](mailto:ying.zhan@tu-darmstadt.de) (Y. Zhan), [ralf.riedel@tu-darmstadt.de](mailto:ralf.riedel@tu-darmstadt.de) (R. Riedel)




Figure S1. SEM images of the (A-D) surface and (a-d) cross-section of D1500-sc, D1800, D2250, D2850 coatings, respectively, cured in ambient environment and temperature for 30 days.